diff -Nru kernel-2.6.28mamba.orig/drivers/net/8139too.c kernel-2.6.28mamba/drivers/net/8139too.c
--- kernel-2.6.28mamba.orig/drivers/net/ethernet/realtek/8139too.c	2008-12-25 00:26:37.000000000 +0100
+++ kernel-2.6.28mamba/drivers/net/ethernet/realtek/8139too.c	2009-10-14 15:09:02.000000000 +0200
@@ -946,9 +946,10 @@
 	if (pdev->vendor == PCI_VENDOR_ID_REALTEK &&
 	    pdev->device == PCI_DEVICE_ID_REALTEK_8139 && pdev->revision >= 0x20) {
 		dev_info(&pdev->dev,
-			   "This (id %04x:%04x rev %02x) is an enhanced 8139C+ chip, use 8139cp\n",
+			   "This (id %04x:%04x rev %02x) is an enhanced 8139C+ chip\n",
 		       	   pdev->vendor, pdev->device, pdev->revision);
-		return -ENODEV;
+		dev_info(&pdev->dev,
+			   "Use the \"8139cp\" driver for improved performance and stability.\n");
 	}
 
 	if (pdev->vendor == PCI_VENDOR_ID_REALTEK &&
